

KRUSHER

MULTI-PURPOSE CLEANER (non-alkaline)

DESCRIPTION

Concentrated tank cleaner with a unique formulation. No other product has any similarity to KRUSHER’s composition. It is often used as a substitute for solvent based cleaners. KRUSHER is non-caustic, non-flammable, non-hazardous and biodegradable. Because of its great emulsifying and deodorizing properties KRUSHER is a good choice for final rinse.

PRODUCT FEATURES

* Will remove residual hydrocarbons from tank linings.
* Good for leaching color/dyes and old detergent residues from tank linings.
* Has brightening effect on stainless steel.
* Powerful deodorizing properties, leaves orange scent.

ZINC CLEANING

Works very well in zinc coated tanks, highly recommended. Cleaning time should be 4-6 hours, at a 2% dilution. Recommended temp range is up to 60 C. A prolonged pre cleaning with water at lower temperature is recommended before using cleaning additives.

METHOD/USE

Works best in a circulation system. A mix of 2%. KRUSHER in water will usually provide good results. It can be used with heat, and works well at 45°-60°C. The length of cleaning time will depend on build-up or degree of staining on tank linings.

PROPERTIES

pH: 9.8 pH (1%): 9.0

SPECIFIC GRAVITY: 1.05

ODOR: Citrus

SOLUBILITY IN WATER: Complete

BIODEGRADEABLE: Yes

APPROVALS

* IMO approved in accordance with MEPC 2.
* Major coating manufacturers

**Stock Points:**

**U.S.A.: South America: Europe: Africa: Asia:**

Houston Panama Rotterdam Egypt Singapore

New York Trinidad