

SUPER GREEN

MULTI-PURPOSE ALKALINE CLEANER

Description

SUPER GREEN is a strong alkaline product that stands out because it has proven to be an exceptional cleaner for a wide variety of cargoes. These include Inert gas stains (IG) soot, vegetable oils, mineral oils, animal fats, and Palm oils.

PRODUCT FEATURES

* Works well on a wide variety of cargoes. (Vegetable oils, Palm Oils, and Soot.)
* High concentrated, works at high dilution rates
* Works well with high pressure equipment, and when used with heat
* Long – lasting, product keeps cleaning until completely expended
* Easy to apply, non-toxic, biodegradable and non-flammable

METHOD/USE

Recirculation: SUPER GREEN can be used with Butterworth or other circulation systems.

SUPER GREEN works especially well when heated, and has a temperature range up to 80°C.

A general recommendation for cleaning vegetable oils, Palm Oils is to use a solution of 2-5% for 2-4 hours, but this rate can vary greatly depending on the cargo and tank size.

SUPER GREEN can be sprayed on neat or diluted on problem areas. Allow 30 minutes dwell time, then rinse.

PROPERTIES

pH: >12

Specific Gravity: 1.05

Flash Point: N/A

Solubility: Complete

APPROVALS

* IMO approved in accordance with MEPC 2.
* Major coating manufacturers

**Stock Points:**

**U.S.A.: South America: Europe: Africa: Asia:**

Houston Panama Rotterdam Egypt Singapore

New York Trinidad