

AQUA-SOLV

TANK CLEANER CONCENTRATE

DESCRIPTION

AQUA-SOLV is an innovative tank cleaner manufactured from natural solvents and raw materials. It contains no aromatic or aliphatic hydrocarbons. It is 100% active, containing no builders or coupling agents. AQUA-SOLV is noted for working well at very low concentrations, and is excellent for cleaning tanks to wall wash standard.

PRODUCT FEATURES

* AQUA-SOLV is designed for cleaning mineral oils, lubricants, oils and greases, paraffin, IG (inert gas) soot, animal oils and fats, crude palm oil, styrene, coal tar and palm fatty acids.
* Highly concentrated, works with low concentration
* Works well when heated in solution. Recommended cleaning temperature is 10-60°C (depending on type of cargo)
* Safe to use, has high flash point
* More effective than aromatics and aliphatics, and much safer

METHOD/USE

Pre-Wash before using AQUA-SOLV, pre-wash the tanks with hot or cold water, depending on the type of cargo.

Re-Circulation Method: Mix AQUA-SOLV in solution at 0.3-0.5% and circulate through the Butterworth system for 4 to 6 hours at a temperature range of 10-60°C (depending on the type of cargo). Spray on neat for problem areas. Allow 30 minutes dwell time, then rinse thoroughly.

PROPERTIES

pH: 9.7

Specific Gravity: 0.096

Flash Point 10%: 72°C

APPROVALS

* IMO approved in accordance with MEPC 2.
* Major coating manufacturers

**Stock Points:**

**U.S.A.: South America: Europe: Africa: Asia:**

Houston Panama Rotterdam Egypt Singapore

New York Trinidad