

CD-SEA

TANK CLEANING CONCENTRATE

FEATURES/APPLICATIONS

* Effective tank cleaning agent for hydrocarbons, lube oils, clean petroleum products (CPP) and, Veg oils.
* Highly concentrated, neutral pH.
* Strong emulsifier, high surface activity.
* No acids, non-alkaline.
* Safe product, non-hazardous/non-dangerous goods.

METHOD/USE

* Can be used in re-circulation cleaning and injected into Butterworth type systems.
* Cleaning temperature range of 10-80°C.
* Cleaning concentration can start as low as 0.2 - 0.5%, and also can be used at higher concentration up to 2%.
* Can be used in fresh water and sea water.

PROPERTIES

Appearance and color: Amber viscous liquid

pH: 7 to 8

Flash Point: Non-flammable

Specific Gravity: 1.02

Solubility in water: Complete

PACKAGING

* 20 Liter pails
* 208 Liter drums

**Stock Points:**

**U.S.A.: South America: Europe: Africa: Asia:**

Houston Panama Rotterdam Egypt Singapore

New York Trinidad