

SEA CLEAN

(IMO APPROVED PRODUCT)

SOLVENT DEGREASER

DESCRIPTION

SEA CLEAN is a hydrocarbon-based compound used to clean heavy oils like crude oil, six-oil, and others, as well as paraffin, asphaltens, and hydrocracker bottoms. Sea Clean will also remove most mineral oils and fats from cargo tank surfaces. Sea Clean is a blend of aliphatic and aromatic solvents compounded with surfactants and wetting agents to make it an aggressive cleaner, even when diluted with water.

PRODUCT FEATURES

* Strong emulsifier and safe to use on common metals
* Cleans by dissolving residues, so extreme agitation is not required
* Product is 100% active, and is water-soluble, allowing economical use in recirculation systems
* Sea Clean can be heated in use-dilution to a range of 60-65°C, increasing its cleaning power
* Product can be used in recirculation, direct injection, spraying on surfaces, and the Sea Clean method

METHOD/USE

Sea Clean can be used by direct injection, recirculation, hand-spraying and the Sea Clean method.

Direct-Injection: Inject 0.1-0.3 Liters of Sea Clean per 100 liters of wash water, this will usually be sufficient.

Recirculation: The recommended solution strength is 2-5% Sea Clean in water. After cleaning, tank should be rinsed, preferably with mild detergent solution.

PROPERTIES

Vapor Pressure: (MMHG -0.1) Specific Gravity: 0.87 Melting Point: 23°F

Reactivity in Water: Emulsifie Flash Point: 85°C, 185°F Odor: Aromatic/Aliphatic

Solubility: Appreciable

**Stock Points:**

**U.S.A.: South America: Europe: Africa: Asia:**

Houston Panama Rotterdam Egypt Singapore

New York Trinidad