

METAL BRIGHT

RUST CLEANER/ACID TANK WASH

DESCRIPTION

METAL BRIGHT is a phosphoric-acid based rust cleaner and pre-paint primer for carbon steel and other ferrous metals. METAL BRIGHT is also used as an acid tank wash to clean the white films left in cargo tanks after alkaline cleaning operations.

PRODUCT FEATURES

* Economical, can be used at low concentrations
* Easy to use, does not require heat to be effective
* Product will clean multiple tanks, until potency is expended (depending on cargo, tank size and degree of soiling).

METHOD/USE

METAL BRIGHT is most often used in recirculation systems for light films or early-stage rusting. A concentration of 1-2% METAL BRIGHT in water will usually get good results. The percentage should be increased for tougher cleaning jobs, in proportion to the amount of residual contamination, staining or streaking.

PROPERTIES

pH: 1-2

Specific Gravity: 1.2 (Water = 1)

Odor/Appearance: Acidic/Clear to Amber Liquid

APPROVALS

* IMO approved in accordance with MEPC 2.
* Major coating manufacturers

**Stock Points:**

**U.S.A.: South America: Europe: Africa: Asia:**

Houston Panama Rotterdam Egypt Singapore

New York Trinidad